NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** UGANDA**If applicable, name of local government involved (Article 3.2 and 7.2):**  |
| **2.** | **Agency responsible:** Uganda National Bureau of StandardsPlot 2-12 ByPass Link, Bweyogerere Industrial and Business ParkP.O. Box 6329Kampala, UgandaTel: +(256) 4 1733 3250/1/2Fax: +(256) 4 1428 6123E-mail: info@unbs.go.ugWebsite: <https://www.unbs.go.ug>**Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:**  |
| **3.** | **Notified under Article 2.9.2 [****X],** **2.10.1 [****],** **5.6.2 [****X],** **5.7.1 [****], 3.2 [****], 7.2 [****],** **other****:**  |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Limestone flux; limestone and other calcareous stone, of a kind used for the manufacture of lime or cement (HS code(s): 2521); Cement. Gypsum. Lime. Mortar (ICS code(s): 91.100.10) |
| **5.** | **Title, number of pages and language(s) of the notified document:** DUS 289: 2022, Limestone for Industrial use — Specification, Second edition; (26 page(s), in English) |
| **6.** | **Description of content:** This Draft Uganda standard specifies the requirements, test methods and sampling of limestone for industrial use. This Draft Uganda Standard does not cover limestone for building, agricultural, metallurgical, glass and ceramic industries. Physical requirements, such as specific gravity, porosity, compressive strength and size of stone are not included in this Draft Uganda Standard, as these requirements will depend on, amongst others, the types of kilns used for burning limestone. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Consumer information, labelling; Prevention of deceptive practices and consumer protection; Protection of human health or safety; Quality requirements; Reducing trade barriers and facilitating trade |
| **8.** | **Relevant documents:** 1. IS 574:1970, glassy sodium metaphosphate — specification
2. IS 3204:1974, Specification for limestone for chemical industry — specification
3. IS 1760:1962, Methods of chemical analysis of limestone, dolomite and allied materials.
4. IS 2109:1962, Methods of sampling dolomite, limestone and other allied materials
5. US EAS 73, Building limes (quicklime and hydrated lime) — Specification
6. US 289: 2001, Specification for Limestone for chemical industries
 |
| **9.** | **Proposed date of adoption:** To be determined**Proposed date of entry into force:** To be determined |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:** Uganda National Bureau of StandardsPlot 2-12 ByPass Link, Bweyogerere Industrial and Business ParkP.O. Box 6329Kampala, UgandaTel: +(256) 4 1733 3250/1/2Fax: +(256) 4 1428 6123E-mail: info@unbs.go.ugWebsite: <https://www.unbs.go.ug><https://members.wto.org/crnattachments/2022/TBT/UGA/22_8520_00_e.pdf> |